



1. Part 22 (Overall dimensions: 4,67 х 3,78 mm, thickness 0,7 mm)
Material: Stainless steel (SST), Roughness, Ra=0,8
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2. Part 23 (Overall dimensions: Ø1 х 5 mm)
Material: Brass (BR)
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3. Part 24 (Overall dimensions: Ø2 x Ø1 x 0,5 mm)
Material: Brass (BR)
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4. Part 25 (Overall dimensions: Ø2 х 1,6 mm)
Material: Brass (BR)
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5. Part 27 (Overall dimensions: Ø3 х 11 mm)
Material: spring-loaded stainless steel (сталь 50ХФА)
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6. Part 28 (Overall dimensions: 8 х 10 х 1,5 mm)
Material: spring-loaded stainless steel (сталь 50ХФА, 12Х18Н10Т)
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7. Part 29 (Overall dimensions: 9 х 5 х 0,3 mm)
Material: Stainless steel (SST)
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8. Part 30 (Overall dimensions: 6,5 х 5 х 0,3 mm)
Material: Stainless steel (SST)
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9. Part 31 (Overall dimensions: 4 х 4 х 0,3 mm)
Material: Stainless steel (SST)
[image: ]


10. Part 32 (Overall dimensions: Ø3 х 11 mm)
Material: spring-loaded stainless steel (сталь 50ХФА, 12Х18Н10Т)
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11. Part 33 (Overall dimensions: 1,2 x 0,3 x 0,2 mm)
Material: Brass (BR)
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12. Part 34 (Overall dimensions: Ø 0,3 x 5,2 mm)
Material: Brass (BR)
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13. Part 35 (Overall dimensions: Ø 0,3 x 1 mm)
Material: Brass (BR)
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14. Part 36 (Overall dimensions: Ø 1 x 2 mm)
Material: magnetic stainless steel (Сталь 40Х13 or AISI 304), Roughness, Ra=0,8
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15. Part 37 (Overall dimensions: 4,79 x 4,1 x 3 mm; thickness 0,1 mm)
Material: spring-loaded stainless steel (сталь 50ХФА, 12Х18Н10Т), Roughness, Ra=0,8
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16. Part 38 (Overall dimensions: 4,58 x 2,14 x 1 mm; thickness 0,1 mm)
Material: spring-loaded stainless steel (сталь 50ХФА, 12Х18Н10Т), Roughness, Ra=0,8
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17. Part 39 (Overall dimensions: Ø 2 x 16,5 mm)
Material: spring-loaded stainless steel (Сталь 40Х13 or AISI 304), Roughness, Ra=0,8…1,6
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18. Part 40 (Overall dimensions: Ø 2 x 16,5 mm)
Material: spring-loaded stainless steel (Сталь 40Х13 or AISI 304), Roughness, Ra=0,8…1,6
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19. Part 41 (Overall dimensions: Ø 0,8 х 7 mm)
Material: spring-loaded stainless steel (Сталь 50ХФА, 12Х18Н10Т)
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20. Part 42 (Overall dimensions: Ø 0,8 х 6 mm)
Material: spring-loaded stainless steel (Сталь 50ХФА, 12Х18Н10Т)
; ; ;  
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21. Part 43 (Overall dimensions: Ø 0,8 х 6 mm)
Material: spring-loaded stainless steel (Сталь 50ХФА, 12Х18Н10Т)
; ; ; ; 
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